Version: V1.3 | Release Date: 2019-11-01

[Process Data]
[Standard Variables]
[Variables]
[ErrorTypes]
[Events]
[Menus]

K50 Pro Device
Vendor ID | 451 (0x01c3) |
Vendor Name | Banner Engineering Corporation
Vendor Text | More Sensors. More Solutions.
Vendor URL | www.bannerengineering.com/io-link
Device ID | 393220 (0x060004)
DeviceFamily | Base Mount Button
Features
Block Parameter | yes
Data Storage | yes
Supported Access Locks | Parameter: yes, Data Storage: yes, Local Parameterization: no, Local User Interface: no
Communication
IO-Link Revision | V1.1
Transmission Rate | 38400 bit/s (COM2)
Minimum Cycle Time | 5 ms
SIO Mode Supported | no
M-Sequence Capability | PREOPERATE = TYPE_0 with 1 octet on-request data OPERATE = TYPE_2_V with 1 octet on-request data ISDU supported
Device Variant | K50PTCKQ
--- | ---
Description | K50 Pro Compact Touch with Euro 4-Pin Quick-Disconnect
Product ID | K50PTCKQ
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Description | IO-Link Euro QD
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
Device Variant | K50PTKQ
Description | K50 Pro Touch with Euro 4-Pin Quick-Disconnect
Product ID | K50PTKQ
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Description | IO-Link Euro QD
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
Device Variant | K50PTCKQP
Description | K50 Pro Compact Touch with Euro 4-pin 150 mm PVC Pigtail Connector
Product ID | K50PTCKQP
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Description | IO-Link Euro QP
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
Device Variant | K50PTKQP
Description | K50 Pro Touch with Euro 4-pin 150 mm PVC Pigtail Connector
Product ID | K50PTKQP
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Description | IO-Link Euro QP
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
Device Variant | K50PTFKQP
Description | K50 Pro Touch with FDA-grade copolyester and Euro 4-pin 150 mm PVC Pigtail Connector
Product ID | K50PTFKQP
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Description | IO-Link Euro QP
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
Device Variant | K50PTVKQ
Description | K50 Pro Touch with Vibration Feedback and Euro 4-Pin Quick-Disconnect
Product ID | K50PTVKQ
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Description | IO-Link Euro QD
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
Device Variant | K50PTVKQP
Description | K50 Pro Touch with Vibration Feedback and Euro 4-pin 150 mm PVC Pigtail Connector
Product ID | K50PTVKQP
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Description | IO-Link Euro QP
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
Device Variant | K50PTFVKQP
Description | K50 Pro Touch with Vibration Feedback, FDA Copolyester, and Euro 4-pin 150 mm PVC Pigtail Connector
Product ID | K50PTFVKQP
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Description | IO-Link Euro QP
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
Device Variant | K50PFF50KQ
Description | K50 Pro 50 mm Optical with Euro 4-Pin Quick-Disconnect
Product ID | K50PFF50KQ
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Description | IO-Link Euro QD
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
Device Variant | K50PFF50KQP
Description | K50 Pro 50 mm Optical with Euro 4-Pin 150 mm PVC Pigtail
Product ID | K50PFF50KQP
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Description | IO-Link Euro QP
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
Device Variant | K50PFF50KQPMA
Description | K50 Pro 50 mm Optical with Euro 4-Pin 150 mm PUR Pigtail
Product ID | K50PFF50KQPMA
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Description | IO-Link Euro QP
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
Device Variant | K50PFF100KQ
Description | K50 Pro 100 mm Optical with Euro 4-Pin Quick-Disconnect
Product ID | K50PFF100KQ
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Description | IO-Link Euro QD
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
Device Variant | K50PFF100KQP
Description | K50 Pro 100 mm Optical with Euro 4-Pin 150 mm PVC Pigtail
Product ID | K50PFF100KQP
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Description | IO-Link Euro QP
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
Device Variant | K50PFF100KQPMA
Description | K50 Pro 100 mm Optical with Euro 4-Pin 150 mm PUR Pigtail
Product ID | K50PFF100KQPMA
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Description | IO-Link Euro QP
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
Device Variant | K50PFF200KQ
Description | K50 Pro 200 mm Optical with Euro 4-Pin Quick-Disconnect
Product ID | K50PFF200KQ
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Description | IO-Link Euro QD
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
Device Variant | K50PFF200KQP
Description | K50 Pro 200 mm Optical with Euro 4-Pin 150 mm PVC Pigtail
Product ID | K50PFF200KQP
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Description | IO-Link Euro QP
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
Device Variant | K50PFF200KQPMA
Description | K50 Pro 200 mm Optical with Euro 4-Pin 150 mm PUR Pigtail
Product ID | K50PFF200KQPMA
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Description | IO-Link Euro QP
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
Device Variant | K50PLVKQ
Description | K50 Pro 200 mm Optical with Euro 4-Pin Quick-Disconnect
Product ID | K50PLVKQ
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Description | IO-Link Euro QD
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
Device Variant | K50PLVKQP
Description | K50 Pro 200 mm Optical with Euro 4-Pin 150 mm PVC Pigtail
Product ID | K50PLVKQP
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Description | IO-Link Euro QP
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
Device Variant | K50PLVKQPMA
Description | K50 Pro 200 mm Optical with Euro 4-Pin 150 mm PUR Pigtail
Product ID | K50PLVKQPMA
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Description | IO-Link Euro QP
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
Device Variant | K50PPBKQ
Description | K50 Pro Push Button with Euro 4-Pin Quick-Disconnect
Product ID | K50PPBKQ
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Description | IO-Link Euro QD
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
Device Variant | K50PPBKQP
Description | K50 Pro Push Button with Euro 4-Pin 150 mm PVC Pigtail
Product ID | K50PPBKQP
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Description | IO-Link Euro QP
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
Device Variant | K50PPBKQPMA
Description | K50 Pro Push Button with Euro 4-Pin 150 mm PUR Pigtail
Product ID | K50PPBKQPMA
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
Connection Description | IO-Link Euro QP
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q

[Top]

## ProcessData id=V_Pd_Multicolor (condition V_OperationMode == 0)

## ProcessDataIn "Process Data In" id=V_Pd_InMulticolor

bit length: 16
data type: 16-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean | false = Inactive, true = Active |  |  |  |  | Output State | Output State. Related parameters defined in output and touch settings parameter data.
2 | 8 | 2-bit UInteger | 0 = State 1, 1 = State 2, 2 = State 3, 3 = State 4 |  |  |  |  | State | Animation State. Related parameters defined in Four State Full Logic/Multicolor parameter data.

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 2
element bit |  |  |  |  |  |  | 1 | 0

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 1

## ProcessDataOut "Process Data Out" id=V_Pd_OutMulticolor

bit length: 80
data type: 80-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 2-bit UInteger | 0 = State1, 1 = State2, 2 = State3, 3 = State4 |  |  |  |  | State | Animation State. Related parameters defined in Four State Full Logic/Multicolor parameter data.

Octet 0

bit offset | 79 | 78 | 77 | 76 | 75 | 74 | 73 | 72
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 1

bit offset | 71 | 70 | 69 | 68 | 67 | 66 | 65 | 64
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 2

bit offset | 63 | 62 | 61 | 60 | 59 | 58 | 57 | 56
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 3

bit offset | 55 | 54 | 53 | 52 | 51 | 50 | 49 | 48
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 4

bit offset | 47 | 46 | 45 | 44 | 43 | 42 | 41 | 40
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 5

bit offset | 39 | 38 | 37 | 36 | 35 | 34 | 33 | 32
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 6

bit offset | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 7

bit offset | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 8

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 9

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 1
element bit |  |  |  |  |  |  | 1 | 0

## ProcessData id=V_Pd_FourStateFullLogic (condition V_OperationMode == 1)

## ProcessDataIn "Process Data In" id=V_Pd_InFourStateFullLogic

bit length: 16
data type: 16-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean | false = Inactive, true = Active |  |  |  |  | Output State | Output State. Related parameters defined in output and touch settings parameter data.
2 | 8 | 2-bit UInteger | 0 = State 1, 1 = State 2, 2 = State 3, 3 = State 4 |  |  |  |  | State | Animation State. Related parameters defined in Four State Full Logic/Multicolor parameter data.

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 2
element bit |  |  |  |  |  |  | 1 | 0

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 1

## ProcessDataOut "Process Data Out" id=V_Pd_OutFourStateFullLogic

bit length: 80
data type: 80-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean | false = Off, true = On |  |  |  |  | Job Input | Job Input for Four State Full Logic mode.

Octet 0

bit offset | 79 | 78 | 77 | 76 | 75 | 74 | 73 | 72
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 1

bit offset | 71 | 70 | 69 | 68 | 67 | 66 | 65 | 64
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 2

bit offset | 63 | 62 | 61 | 60 | 59 | 58 | 57 | 56
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 3

bit offset | 55 | 54 | 53 | 52 | 51 | 50 | 49 | 48
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 4

bit offset | 47 | 46 | 45 | 44 | 43 | 42 | 41 | 40
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 5

bit offset | 39 | 38 | 37 | 36 | 35 | 34 | 33 | 32
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 6

bit offset | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 7

bit offset | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 8

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 9

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 1

## ProcessData id=V_Pd_Advanced (condition V_OperationMode == 2)

## ProcessDataIn "Process Data In" id=V_Pd_InAdvanced

bit length: 16
data type: 16-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean | false = Inactive, true = Active |  |  |  |  | Output State | Output State. Related parameters defined in output and touch settings parameter data.

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 1

## ProcessDataOut "Process Data Out" id=V_Pd_OutAdvanced

bit length: 80
data type: 80-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 4-bit UInteger | 0 = Off, 1 = Steady, 2 = Flash, 3 = Two Color Flash, 4 = 50/50, 5 = 50/50 Rotate, 6 = Chase, 7 = Intensity Sweep, 8 = Color Sweep, 9 = Sequence |  |  |  |  | Animation Type | The Animation type
2 | 4 | Boolean | false = CCW, true = CW |  |  |  |  | Animation Direction | The Direction of Animation rotation
3 | 5 | 3-bit UInteger | 0 = Flash, 1 = Strobe, 2 = Three Pulse, 3 = SOS, 4 = Random |  |  |  |  | Animation Pattern | The pattern of Animation/Vibration Feedback
4 | 8 | 2-bit UInteger | 0 = Slow, 1 = Medium, 2 = Fast, 3 = Custom |  |  |  |  | Animation Speed | The speed of the Animation/Vibration Feedback
5 | 10 | 2-bit UInteger | 0 = Off, 1 = On, 2 = Animation Pattern |  |  |  |  | Vibration Feedback | Type of Vibration Feedback
6 | 32 | 8-bit UInteger | 0..255 |  |  |  |  | Dynamic Sequence Value (0-255) | Value describing the LED position of the device. LED states defined in process data.
7 | 40 | 3-bit UInteger | 0 = LED1, 1 = LED2, 2 = LED3, 3 = LED4, 4 = LED5, 5 = LED6, 6 = LED7, 7 = LED8 |  |  |  |  | Sequence Start Location | Defines the LED location that the sequence animation is initiated at.
8 | 48 | 5-bit UInteger | 0 = Green, 1 = Red, 2 = Orange, 3 = Amber, 4 = Yellow, 5 = Lime Green, 6 = Spring Green, 7 = Cyan, 8 = Sky Blue, 9 = Blue, 10 = Violet, 11 = Magenta, 12 = Rose, 13 = White, 14 = Custom1, 15 = Custom2 |  |  |  |  | Color 1 | The main color of the Animation, Custom Colors are defined in Parameter data
9 | 53 | 3-bit UInteger | 0 = High, 1 = Medium, 2 = Low, 3 = Off, 4 = Custom |  |  |  |  | Color 1 Intensity | The Intensity of Color 1, Custom Intensity defined in Parameter Data
10 | 56 | 5-bit UInteger | 0 = Green, 1 = Red, 2 = Orange, 3 = Amber, 4 = Yellow, 5 = Lime Green, 6 = Spring Green, 7 = Cyan, 8 = Sky Blue, 9 = Blue, 10 = Violet, 11 = Magenta, 12 = Rose, 13 = White, 14 = Custom1, 15 = Custom2 |  |  |  |  | Color 2 | The secondary color of the Animation, Custom Colors are defined in Parameter data
11 | 61 | 3-bit UInteger | 0 = High, 1 = Medium, 2 = Low, 3 = Off, 4 = Custom |  |  |  |  | Color 2 Intensity | The Intensity of Color 2, Custom Intensity defined in Parameter Data

Octet 0

bit offset | 79 | 78 | 77 | 76 | 75 | 74 | 73 | 72
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 1

bit offset | 71 | 70 | 69 | 68 | 67 | 66 | 65 | 64
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 2

bit offset | 63 | 62 | 61 | 60 | 59 | 58 | 57 | 56
subindex | 11 | 10
element bit | 2 | 1 | 0 | 4 | 3 | 2 | 1 | 0

Octet 3

bit offset | 55 | 54 | 53 | 52 | 51 | 50 | 49 | 48
subindex | 9 | 8
element bit | 2 | 1 | 0 | 4 | 3 | 2 | 1 | 0

Octet 4

bit offset | 47 | 46 | 45 | 44 | 43 | 42 | 41 | 40
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 7
element bit |  |  |  |  |  | 2 | 1 | 0

Octet 5

bit offset | 39 | 38 | 37 | 36 | 35 | 34 | 33 | 32
subindex | 6
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 6

bit offset | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 7

bit offset | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 8

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 5 | 4
element bit |  |  |  |  | 1 | 0 | 1 | 0

Octet 9

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | 3 | 2 | 1
element bit | 2 | 1 | 0 |  | 3 | 2 | 1 | 0

## ProcessData id=V_Pd_LedControl (condition V_OperationMode == 3)

## ProcessDataIn "Process Data In" id=V_Pd_InLedControl

bit length: 16
data type: 16-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean | false = Inactive, true = Active |  |  |  |  | Output State | Output State. Related parameters defined in output and touch settings parameter data.

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 1

## ProcessDataOut "Process Data Out" id=V_Pd_OutLedControl

bit length: 80
data type: 80-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 4-bit UInteger | 0 = Green, 1 = Red, 2 = Orange, 3 = Amber, 4 = Yellow, 5 = Lime Green, 6 = Spring Green, 7 = Cyan, 8 = Sky Blue, 9 = Blue, 10 = Violet, 11 = Magenta, 12 = Rose, 13 = White, 14 = Custom1, 15 = Custom2 |  |  |  |  | LED 1 Color | Defines the color of the designated LED. LED 1 is oriented at the 12 O'clock position
2 | 4 | 4-bit UInteger | 0..10 |  |  |  |  | LED 1 Intensity (0-10) | Defines the intensity of the designated LED
3 | 8 | 4-bit UInteger | 0 = Green, 1 = Red, 2 = Orange, 3 = Amber, 4 = Yellow, 5 = Lime Green, 6 = Spring Green, 7 = Cyan, 8 = Sky Blue, 9 = Blue, 10 = Violet, 11 = Magenta, 12 = Rose, 13 = White, 14 = Custom1, 15 = Custom2 |  |  |  |  | LED 2 Color | Defines the color of the designated LED
4 | 12 | 4-bit UInteger | 0..10 |  |  |  |  | LED 2 Intensity (0-10) | Defines the intensity of the designated LED
5 | 16 | 4-bit UInteger | 0 = Green, 1 = Red, 2 = Orange, 3 = Amber, 4 = Yellow, 5 = Lime Green, 6 = Spring Green, 7 = Cyan, 8 = Sky Blue, 9 = Blue, 10 = Violet, 11 = Magenta, 12 = Rose, 13 = White, 14 = Custom1, 15 = Custom2 |  |  |  |  | LED 3 Color | Defines the color of the designated LED
6 | 20 | 4-bit UInteger | 0..10 |  |  |  |  | LED 3 Intensity (0-10) | Defines the intensity of the designated LED
7 | 24 | 4-bit UInteger | 0 = Green, 1 = Red, 2 = Orange, 3 = Amber, 4 = Yellow, 5 = Lime Green, 6 = Spring Green, 7 = Cyan, 8 = Sky Blue, 9 = Blue, 10 = Violet, 11 = Magenta, 12 = Rose, 13 = White, 14 = Custom1, 15 = Custom2 |  |  |  |  | LED 4 Color | Defines the color of the designated LED
8 | 28 | 4-bit UInteger | 0..10 |  |  |  |  | LED 4 Intensity (0-10) | Defines the intensity of the designated LED
9 | 32 | 4-bit UInteger | 0 = Green, 1 = Red, 2 = Orange, 3 = Amber, 4 = Yellow, 5 = Lime Green, 6 = Spring Green, 7 = Cyan, 8 = Sky Blue, 9 = Blue, 10 = Violet, 11 = Magenta, 12 = Rose, 13 = White, 14 = Custom1, 15 = Custom2 |  |  |  |  | LED 5 Color | Defines the color of the designated LED
10 | 36 | 4-bit UInteger | 0..10 |  |  |  |  | LED 5 Intensity (0-10) | Defines the intensity of the designated LED
11 | 40 | 4-bit UInteger | 0 = Green, 1 = Red, 2 = Orange, 3 = Amber, 4 = Yellow, 5 = Lime Green, 6 = Spring Green, 7 = Cyan, 8 = Sky Blue, 9 = Blue, 10 = Violet, 11 = Magenta, 12 = Rose, 13 = White, 14 = Custom1, 15 = Custom2 |  |  |  |  | LED 6 Color | Defines the color of the designated LED
12 | 44 | 4-bit UInteger | 0..10 |  |  |  |  | LED 6 Intensity (0-10) | Defines the intensity of the designated LED
13 | 48 | 4-bit UInteger | 0 = Green, 1 = Red, 2 = Orange, 3 = Amber, 4 = Yellow, 5 = Lime Green, 6 = Spring Green, 7 = Cyan, 8 = Sky Blue, 9 = Blue, 10 = Violet, 11 = Magenta, 12 = Rose, 13 = White, 14 = Custom1, 15 = Custom2 |  |  |  |  | LED 8 Color | Defines the color of the designated LED
14 | 52 | 4-bit UInteger | 0..10 |  |  |  |  | LED 7 Intensity (0-10) | Defines the intensity of the designated LED
15 | 56 | 4-bit UInteger | 0 = Green, 1 = Red, 2 = Orange, 3 = Amber, 4 = Yellow, 5 = Lime Green, 6 = Spring Green, 7 = Cyan, 8 = Sky Blue, 9 = Blue, 10 = Violet, 11 = Magenta, 12 = Rose, 13 = White, 14 = Custom1, 15 = Custom2 |  |  |  |  | LED 8 Color | Defines the color of the designated LED
16 | 60 | 4-bit UInteger | 0..10 |  |  |  |  | LED 8 Intensity (0-10) | Defines the intensity of the designated LED
17 | 64 | 2-bit UInteger | 0 = Off, 1 = On, 2 = Pattern |  |  |  |  | Vibration Feedback |
18 | 66 | 3-bit UInteger | 0 = Flash, 1 = Strobe, 2 = Three Pulse, 3 = SOS, 4 = Random |  |  |  |  | Vibration Pattern |
19 | 69 | 2-bit UInteger | 0 = Slow, 1 = Medium, 2 = Fast, 3 = Custom |  |  |  |  | Vibration Speed |

Octet 0

bit offset | 79 | 78 | 77 | 76 | 75 | 74 | 73 | 72
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 1

bit offset | 71 | 70 | 69 | 68 | 67 | 66 | 65 | 64
subindex | / / / / / / | 19 | 18 | 17
element bit |  | 1 | 0 | 2 | 1 | 0 | 1 | 0

Octet 2

bit offset | 63 | 62 | 61 | 60 | 59 | 58 | 57 | 56
subindex | 16 | 15
element bit | 3 | 2 | 1 | 0 | 3 | 2 | 1 | 0

Octet 3

bit offset | 55 | 54 | 53 | 52 | 51 | 50 | 49 | 48
subindex | 14 | 13
element bit | 3 | 2 | 1 | 0 | 3 | 2 | 1 | 0

Octet 4

bit offset | 47 | 46 | 45 | 44 | 43 | 42 | 41 | 40
subindex | 12 | 11
element bit | 3 | 2 | 1 | 0 | 3 | 2 | 1 | 0

Octet 5

bit offset | 39 | 38 | 37 | 36 | 35 | 34 | 33 | 32
subindex | 10 | 9
element bit | 3 | 2 | 1 | 0 | 3 | 2 | 1 | 0

Octet 6

bit offset | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
subindex | 8 | 7
element bit | 3 | 2 | 1 | 0 | 3 | 2 | 1 | 0

Octet 7

bit offset | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
subindex | 6 | 5
element bit | 3 | 2 | 1 | 0 | 3 | 2 | 1 | 0

Octet 8

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | 4 | 3
element bit | 3 | 2 | 1 | 0 | 3 | 2 | 1 | 0

Octet 9

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | 2 | 1
element bit | 3 | 2 | 1 | 0 | 3 | 2 | 1 | 0

[Top]

## Standard Variable "Direct Parameters 1" index=0 id=V_DirectParameters_1

data type: 128-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  | ro |  |  | Reserved |
2 | 112 | 8-bit UInteger |  |  | ro |  |  | Master Cycle Time |
3 | 104 | 8-bit UInteger |  |  | ro |  |  | Min Cycle Time |
4 | 96 | 8-bit UInteger |  |  | ro |  |  | M-Sequence Capability |
5 | 88 | 8-bit UInteger |  | 17 | ro |  |  | IO-Link Version ID |
6 | 80 | 8-bit UInteger |  |  | ro |  |  | Process Data Input Length |
7 | 72 | 8-bit UInteger |  |  | ro |  |  | Process Data Output Length |
8 | 64 | 8-bit UInteger |  |  | ro |  |  | Vendor ID 1 |
9 | 56 | 8-bit UInteger |  |  | ro |  |  | Vendor ID 2 |
10 | 48 | 8-bit UInteger |  |  | ro |  |  | Device ID 1 |
11 | 40 | 8-bit UInteger |  |  | ro |  |  | Device ID 2 |
12 | 32 | 8-bit UInteger |  |  | ro |  |  | Device ID 3 |
13 | 24 | 8-bit UInteger |  |  | ro |  |  | Reserved |
14 | 16 | 8-bit UInteger |  |  | ro |  |  | Reserved |
15 | 8 | 8-bit UInteger |  |  | ro |  |  | Reserved |
16 | 0 | 8-bit UInteger | 130 = Restore Factory Settings |  | wo | X |  | Standard Command |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "Direct Parameters 2" index=1 id=V_DirectParameters_2

data type: 128-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 1 |
2 | 112 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 2 |
3 | 104 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 3 |
4 | 96 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 4 |
5 | 88 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 5 |
6 | 80 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 6 |
7 | 72 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 7 |
8 | 64 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 8 |
9 | 56 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 9 |
10 | 48 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 10 |
11 | 40 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 11 |
12 | 32 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 12 |
13 | 24 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 13 |
14 | 16 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 14 |
15 | 8 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 15 |
16 | 0 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 16 |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "Standard Command" index=2 id=V_SystemCommand

data type: 8-bit UInteger
allowed values: 130 = Restore Factory Settings
access rights: wo
modifies other variables

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Standard Variable "Device Access Locks" index=12 id=V_DeviceAccessLocks

data type: 16-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean |  | false |  |  |  | Parameter (write) Access Lock |
2 | 1 | Boolean |  | false |  |  |  | Data Storage Lock |
3 | 2 | Boolean |  |  |  |  |  | Local Parameterization Lock |
4 | 3 | Boolean |  |  |  |  |  | Local User Interface Lock |

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 4 | 3 | 2 | 1

## Standard Variable "Vendor Name" index=16 id=V_VendorName

data type: 30-octet String UTF-8
default value: "Banner Engineering Corporation"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192 | 191 - 184 | 183 - 176

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128 | 127 - 120 | 119 - 112

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48

octet | 24 | 25 | 26 | 27 | 28 | 29 |
bit offset | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Standard Variable "Vendor Text" index=17 id=V_VendorText

data type: 29-octet String UTF-8
default value: "More Sensors. More Solutions."
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192 | 191 - 184 | 183 - 176 | 175 - 168

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128 | 127 - 120 | 119 - 112 | 111 - 104

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40

octet | 24 | 25 | 26 | 27 | 28 |
bit offset | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Standard Variable "Product Name" index=18 id=V_ProductName

data type: 32-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product ID" index=19 id=V_ProductID

data type: 32-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Text" index=20 id=V_ProductText

data type: 27-octet String UTF-8
default value: "K50 Pro Device with IO-Link"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 215 - 208 | 207 - 200 | 199 - 192 | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 151 - 144 | 143 - 136 | 135 - 128 | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24

octet | 24 | 25 | 26 |
bit offset | 23 - 16 | 15 - 8 | 7 - 0 |

## Standard Variable "Serial Number" index=21 id=V_SerialNumber

data type: 16-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Hardware Version" index=22 id=V_HardwareRevision

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Firmware Version" index=23 id=V_FirmwareRevision

data type: 8-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Application Specific Tag" index=24 id=V_ApplicationSpecificTag

data type: 32-octet String UTF-8
access rights: rw

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Device Status" index=36 id=V_DeviceStatus

data type: 8-bit UInteger
allowed values: 0 = Device is OK, 1 = Maintenance required, 2 = Out of specification, 3 = Functional check, 4 = Failure, 5..255 = Reserved
access rights: ro
dynamic

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Standard Variable "Detailed Device Status" index=37 id=V_DetailedDeviceStatus

data type: Array[6] of 3-octet OctetString (subindex access not supported)
access rights: ro
dynamic

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 143 - 136 | 135 - 128 | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80
subindex | 1 | 1 | 1 | 2 | 2 | 2 | 3 | 3

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16
subindex | 3 | 4 | 4 | 4 | 5 | 5 | 5 | 6

octet | 16 | 17 |
bit offset | 15 - 8 | 7 - 0 |
subindex | 6 | 6 |

[Top]

## Variable "Operation Mode" index=80 id=V_OperationMode

description: Operation Mode
data type: 3-bit UInteger
allowed values: 0 = Multicolor, 1 = Four State Full Logic, 2 = Advanced, 3 = LED Control, 4 = Demo
default value: 2
access rights: rw
Octet 0

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
element bit | null ext. | 2 | 1 | 0

## Variable "Setting" index=81 id=V_CustomAnimationSettings

description: Setting
data type: 24-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0..100 | 100 |  |  |  | Custom Intensity (0 - 100%) | Set custom intensity to be used
2 | 8 | 8-bit UInteger | 5..255 | 15 |  |  |  | Custom Flash Rate (0.5 - 25.5 Hz) | Set custom flash rate to be used
3 | 16 | 8-bit UInteger | 0 = Off, 1 = On | 0 |  |  |  | Restrict To Gamut | Turn on to show more consistent colors from device to device

octet | 0 | 1 | 2 |
bit offset | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 2 | 1 |
element bit | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Touch Settings" index=82 id=V_InputSettings

description: Touch Settings
data type: 24-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 2-bit UInteger | 0 = Low, 1 = Standard, 2 = High | 1 |  |  |  | Touch Sensitivity | Defines the sensitivity of the touch button. High sensitivity will allow easier actuation. Low sensitivity will prevent false actuation.
2 | 2 | Boolean | false = Momentary, true = Latched | false |  |  |  | Function | In Momentary mode, output is active only while the button is touched. In Latching mode, output is activate each time the button is pressed.
3 | 3 | Boolean | false = Off, true = On | false |  |  |  | Mute Enable | Prevents the touch input from activating the output.
4 | 8 | 16-bit UInteger | 0..65535 | 0 |  |  |  | On Delay (ms) | Length of time the touch button needs to be pressed to trigger 'touch active' state.

Octet 0

bit offset | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
subindex | 4
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 1

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | 4
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 2

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 3 | 2 | 1
element bit |  |  |  |  |  |  | 1 | 0

## Variable "Output Settings" index=83 id=V_OutputSettings

description: Output Settings
data type: 24-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean | false = Normally Closed, true = Normally Open | true |  |  |  | Output State | When defined as normally open, the output is active with a touch input. When defined as normally closed, the output is inactive with a touch input.
2 | 1 | Boolean | false = Leading Edge, true = Trailing Edge | false |  |  |  | Off Delay Type | A leading edge delay is triggered on the rising edge of a touch input. A trailing edge delay is triggered on a the falling edge of a touch input.
3 | 8 | 16-bit UInteger | 0..65535 | 0 |  |  |  | Off Delay (ms) | Length of time before the device returns to 'touch inactive' state after button is released.

Octet 0

bit offset | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
subindex | 3
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 1

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | 3
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 2

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 2 | 1

## Variable "State 1 Parameters" index=84 id=V_StateParameters1

description: State 1 Parameters
data type: 64-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 4-bit UInteger | 0 = Off, 1 = Steady, 2 = Flash, 3 = Two Color Flash, 4 = 50/50, 5 = 50/50 Rotate, 6 = Chase, 7 = Intensity Sweep, 8 = Color Sweep, 9 = Sequence | 1 |  |  |  | Animation Type | The Animation type
2 | 4 | Boolean | false = CCW, true = CW | false |  |  |  | Animation Direction | The Direction of Animation rotation
3 | 5 | 3-bit UInteger | 0 = Flash, 1 = Strobe, 2 = Three Pulse, 3 = SOS, 4 = Random | 0 |  |  |  | Animation Pattern | The pattern of Animation/Vibration Feedback
4 | 8 | 2-bit UInteger | 0 = Slow, 1 = Medium, 2 = Fast, 3 = Custom | 1 |  |  |  | Animation Speed | The speed of the Animation/Vibration Feedback
5 | 10 | 2-bit UInteger | 0 = Off, 1 = On, 2 = Animation Pattern | 1 |  |  |  | Vibration Feedback | Type of Vibration Feedback
6 | 12 | Boolean | false = Leading Edge, true = Trailing Edge | false |  |  |  | Off Delay Type | A leading edge delay is triggered on the rising edge of a touch input. A trailing edge delay is triggered on a the falling edge of a touch input.
7 | 16 | 16-bit UInteger | 0..65535 | 0 |  |  |  | Off Delay (ms) | Length of time before the device returns to 'touch inactive' state after button is released.
8 | 32 | 8-bit UInteger | 0..255 | 0 |  |  |  | Static Sequence Value (0-255) | Value describing the LED position of the device. LED state defined in parameter data.
9 | 40 | 3-bit UInteger | 0 = LED1, 1 = LED2, 2 = LED3, 3 = LED4, 4 = LED5, 5 = LED6, 6 = LED7, 7 = LED8 | 0 |  |  |  | Sequence Start Location | Defines the LED location that the sequence animation is initiated at.
10 | 48 | 5-bit UInteger | 0 = Green, 1 = Red, 2 = Orange, 3 = Amber, 4 = Yellow, 5 = Lime Green, 6 = Spring Green, 7 = Cyan, 8 = Sky Blue, 9 = Blue, 10 = Violet, 11 = Magenta, 12 = Rose, 13 = White, 14 = Custom1, 15 = Custom2 | 0 |  |  |  | Color 1 | The main color of the Animation, Custom Colors are defined in Parameter data
11 | 53 | 3-bit UInteger | 0 = High, 1 = Medium, 2 = Low, 3 = Off, 4 = Custom | 0 |  |  |  | Color 1 Intensity | The Intensity of Color 1, Custom Intensity defined in Parameter Data
12 | 56 | 5-bit UInteger | 0 = Green, 1 = Red, 2 = Orange, 3 = Amber, 4 = Yellow, 5 = Lime Green, 6 = Spring Green, 7 = Cyan, 8 = Sky Blue, 9 = Blue, 10 = Violet, 11 = Magenta, 12 = Rose, 13 = White, 14 = Custom1, 15 = Custom2 | 0 |  |  |  | Color 2 | The secondary color of the Animation, Custom Colors are defined in Parameter data
13 | 61 | 3-bit UInteger | 0 = High, 1 = Medium, 2 = Low, 3 = Off, 4 = Custom | 0 |  |  |  | Color 2 Intensity | The Intensity of Color 2, Custom Intensity defined in Parameter Data

Octet 0

bit offset | 63 | 62 | 61 | 60 | 59 | 58 | 57 | 56
subindex | 13 | 12
element bit | 2 | 1 | 0 | 4 | 3 | 2 | 1 | 0

Octet 1

bit offset | 55 | 54 | 53 | 52 | 51 | 50 | 49 | 48
subindex | 11 | 10
element bit | 2 | 1 | 0 | 4 | 3 | 2 | 1 | 0

Octet 2

bit offset | 47 | 46 | 45 | 44 | 43 | 42 | 41 | 40
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 9
element bit |  |  |  |  |  | 2 | 1 | 0

Octet 3

bit offset | 39 | 38 | 37 | 36 | 35 | 34 | 33 | 32
subindex | 8
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 4

bit offset | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
subindex | 7
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 5

bit offset | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
subindex | 7
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 6

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | 6 | 5 | 4
element bit |  |  |  |  | 1 | 0 | 1 | 0

Octet 7

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | 3 | 2 | 1
element bit | 2 | 1 | 0 |  | 3 | 2 | 1 | 0

## Variable "State 2 Parameters" index=85 id=V_StateParameters2

description: State 2 Parameters
data type: 64-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 4-bit UInteger | 0 = Off, 1 = Steady, 2 = Flash, 3 = Two Color Flash, 4 = 50/50, 5 = 50/50 Rotate, 6 = Chase, 7 = Intensity Sweep, 8 = Color Sweep, 9 = Sequence | 1 |  |  |  | Animation Type | The Animation type
2 | 4 | Boolean | false = CCW, true = CW | false |  |  |  | Animation Direction | The Direction of Animation rotation
3 | 5 | 3-bit UInteger | 0 = Flash, 1 = Strobe, 2 = Three Pulse, 3 = SOS, 4 = Random | 0 |  |  |  | Animation Pattern | The pattern of Animation/Vibration Feedback
4 | 8 | 2-bit UInteger | 0 = Slow, 1 = Medium, 2 = Fast, 3 = Custom | 1 |  |  |  | Animation Speed | The speed of the Animation/Vibration Feedback
5 | 10 | 2-bit UInteger | 0 = Off, 1 = On, 2 = Animation Pattern | 1 |  |  |  | Vibration Feedback | Type of Vibration Feedback
6 | 12 | Boolean | false = Leading Edge, true = Trailing Edge | false |  |  |  | Off Delay Type | A leading edge delay is triggered on the rising edge of a touch input. A trailing edge delay is triggered on a the falling edge of a touch input.
7 | 16 | 16-bit UInteger | 0..65535 | 0 |  |  |  | Off Delay (ms) | Length of time before the device returns to 'touch inactive' state after button is released.
8 | 32 | 8-bit UInteger | 0..255 | 0 |  |  |  | Static Sequence Value (0-255) | Value describing the LED position of the device. LED state defined in parameter data.
9 | 40 | 3-bit UInteger | 0 = LED1, 1 = LED2, 2 = LED3, 3 = LED4, 4 = LED5, 5 = LED6, 6 = LED7, 7 = LED8 | 0 |  |  |  | Sequence Start Location | Defines the LED location that the sequence animation is initiated at.
10 | 48 | 5-bit UInteger | 0 = Green, 1 = Red, 2 = Orange, 3 = Amber, 4 = Yellow, 5 = Lime Green, 6 = Spring Green, 7 = Cyan, 8 = Sky Blue, 9 = Blue, 10 = Violet, 11 = Magenta, 12 = Rose, 13 = White, 14 = Custom1, 15 = Custom2 | 0 |  |  |  | Color 1 | The main color of the Animation, Custom Colors are defined in Parameter data
11 | 53 | 3-bit UInteger | 0 = High, 1 = Medium, 2 = Low, 3 = Off, 4 = Custom | 0 |  |  |  | Color 1 Intensity | The Intensity of Color 1, Custom Intensity defined in Parameter Data
12 | 56 | 5-bit UInteger | 0 = Green, 1 = Red, 2 = Orange, 3 = Amber, 4 = Yellow, 5 = Lime Green, 6 = Spring Green, 7 = Cyan, 8 = Sky Blue, 9 = Blue, 10 = Violet, 11 = Magenta, 12 = Rose, 13 = White, 14 = Custom1, 15 = Custom2 | 0 |  |  |  | Color 2 | The secondary color of the Animation, Custom Colors are defined in Parameter data
13 | 61 | 3-bit UInteger | 0 = High, 1 = Medium, 2 = Low, 3 = Off, 4 = Custom | 0 |  |  |  | Color 2 Intensity | The Intensity of Color 2, Custom Intensity defined in Parameter Data

Octet 0

bit offset | 63 | 62 | 61 | 60 | 59 | 58 | 57 | 56
subindex | 13 | 12
element bit | 2 | 1 | 0 | 4 | 3 | 2 | 1 | 0

Octet 1

bit offset | 55 | 54 | 53 | 52 | 51 | 50 | 49 | 48
subindex | 11 | 10
element bit | 2 | 1 | 0 | 4 | 3 | 2 | 1 | 0

Octet 2

bit offset | 47 | 46 | 45 | 44 | 43 | 42 | 41 | 40
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 9
element bit |  |  |  |  |  | 2 | 1 | 0

Octet 3

bit offset | 39 | 38 | 37 | 36 | 35 | 34 | 33 | 32
subindex | 8
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 4

bit offset | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
subindex | 7
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 5

bit offset | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
subindex | 7
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 6

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | 6 | 5 | 4
element bit |  |  |  |  | 1 | 0 | 1 | 0

Octet 7

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | 3 | 2 | 1
element bit | 2 | 1 | 0 |  | 3 | 2 | 1 | 0

## Variable "State 3 Parameters" index=86 id=V_StateParameters3

description: State 3 Parameters
data type: 64-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 4-bit UInteger | 0 = Off, 1 = Steady, 2 = Flash, 3 = Two Color Flash, 4 = 50/50, 5 = 50/50 Rotate, 6 = Chase, 7 = Intensity Sweep, 8 = Color Sweep, 9 = Sequence | 1 |  |  |  | Animation Type | The Animation type
2 | 4 | Boolean | false = CCW, true = CW | false |  |  |  | Animation Direction | The Direction of Animation rotation
3 | 5 | 3-bit UInteger | 0 = Flash, 1 = Strobe, 2 = Three Pulse, 3 = SOS, 4 = Random | 0 |  |  |  | Animation Pattern | The pattern of Animation/Vibration Feedback
4 | 8 | 2-bit UInteger | 0 = Slow, 1 = Medium, 2 = Fast, 3 = Custom | 1 |  |  |  | Animation Speed | The speed of the Animation/Vibration Feedback
5 | 10 | 2-bit UInteger | 0 = Off, 1 = On, 2 = Animation Pattern | 1 |  |  |  | Vibration Feedback | Type of Vibration Feedback
6 | 12 | Boolean | false = Leading Edge, true = Trailing Edge | false |  |  |  | Off Delay Type | A leading edge delay is triggered on the rising edge of a touch input. A trailing edge delay is triggered on a the falling edge of a touch input.
7 | 16 | 16-bit UInteger | 0..65535 | 0 |  |  |  | Off Delay (ms) | Length of time before the device returns to 'touch inactive' state after button is released.
8 | 32 | 8-bit UInteger | 0..255 | 0 |  |  |  | Static Sequence Value (0-255) | Value describing the LED position of the device. LED state defined in parameter data.
9 | 40 | 3-bit UInteger | 0 = LED1, 1 = LED2, 2 = LED3, 3 = LED4, 4 = LED5, 5 = LED6, 6 = LED7, 7 = LED8 | 0 |  |  |  | Sequence Start Location | Defines the LED location that the sequence animation is initiated at.
10 | 48 | 5-bit UInteger | 0 = Green, 1 = Red, 2 = Orange, 3 = Amber, 4 = Yellow, 5 = Lime Green, 6 = Spring Green, 7 = Cyan, 8 = Sky Blue, 9 = Blue, 10 = Violet, 11 = Magenta, 12 = Rose, 13 = White, 14 = Custom1, 15 = Custom2 | 0 |  |  |  | Color 1 | The main color of the Animation, Custom Colors are defined in Parameter data
11 | 53 | 3-bit UInteger | 0 = High, 1 = Medium, 2 = Low, 3 = Off, 4 = Custom | 0 |  |  |  | Color 1 Intensity | The Intensity of Color 1, Custom Intensity defined in Parameter Data
12 | 56 | 5-bit UInteger | 0 = Green, 1 = Red, 2 = Orange, 3 = Amber, 4 = Yellow, 5 = Lime Green, 6 = Spring Green, 7 = Cyan, 8 = Sky Blue, 9 = Blue, 10 = Violet, 11 = Magenta, 12 = Rose, 13 = White, 14 = Custom1, 15 = Custom2 | 0 |  |  |  | Color 2 | The secondary color of the Animation, Custom Colors are defined in Parameter data
13 | 61 | 3-bit UInteger | 0 = High, 1 = Medium, 2 = Low, 3 = Off, 4 = Custom | 0 |  |  |  | Color 2 Intensity | The Intensity of Color 2, Custom Intensity defined in Parameter Data

Octet 0

bit offset | 63 | 62 | 61 | 60 | 59 | 58 | 57 | 56
subindex | 13 | 12
element bit | 2 | 1 | 0 | 4 | 3 | 2 | 1 | 0

Octet 1

bit offset | 55 | 54 | 53 | 52 | 51 | 50 | 49 | 48
subindex | 11 | 10
element bit | 2 | 1 | 0 | 4 | 3 | 2 | 1 | 0

Octet 2

bit offset | 47 | 46 | 45 | 44 | 43 | 42 | 41 | 40
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 9
element bit |  |  |  |  |  | 2 | 1 | 0

Octet 3

bit offset | 39 | 38 | 37 | 36 | 35 | 34 | 33 | 32
subindex | 8
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 4

bit offset | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
subindex | 7
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 5

bit offset | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
subindex | 7
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 6

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | 6 | 5 | 4
element bit |  |  |  |  | 1 | 0 | 1 | 0

Octet 7

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | 3 | 2 | 1
element bit | 2 | 1 | 0 |  | 3 | 2 | 1 | 0

## Variable "State 4 Parameters" index=87 id=V_StateParameters4

description: State 4 Parameters
data type: 64-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 4-bit UInteger | 0 = Off, 1 = Steady, 2 = Flash, 3 = Two Color Flash, 4 = 50/50, 5 = 50/50 Rotate, 6 = Chase, 7 = Intensity Sweep, 8 = Color Sweep, 9 = Sequence | 1 |  |  |  | Animation Type | The Animation type
2 | 4 | Boolean | false = CCW, true = CW | false |  |  |  | Animation Direction | The Direction of Animation rotation
3 | 5 | 3-bit UInteger | 0 = Flash, 1 = Strobe, 2 = Three Pulse, 3 = SOS, 4 = Random | 0 |  |  |  | Animation Pattern | The pattern of Animation/Vibration Feedback
4 | 8 | 2-bit UInteger | 0 = Slow, 1 = Medium, 2 = Fast, 3 = Custom | 1 |  |  |  | Animation Speed | The speed of the Animation/Vibration Feedback
5 | 10 | 2-bit UInteger | 0 = Off, 1 = On, 2 = Animation Pattern | 1 |  |  |  | Vibration Feedback | Type of Vibration Feedback
6 | 12 | Boolean | false = Leading Edge, true = Trailing Edge | false |  |  |  | Off Delay Type | A leading edge delay is triggered on the rising edge of a touch input. A trailing edge delay is triggered on a the falling edge of a touch input.
7 | 16 | 16-bit UInteger | 0..65535 | 0 |  |  |  | Off Delay (ms) | Length of time before the device returns to 'touch inactive' state after button is released.
8 | 32 | 8-bit UInteger | 0..255 | 0 |  |  |  | Static Sequence Value (0-255) | Value describing the LED position of the device. LED state defined in parameter data.
9 | 40 | 3-bit UInteger | 0 = LED1, 1 = LED2, 2 = LED3, 3 = LED4, 4 = LED5, 5 = LED6, 6 = LED7, 7 = LED8 | 0 |  |  |  | Sequence Start Location | Defines the LED location that the sequence animation is initiated at.
10 | 48 | 5-bit UInteger | 0 = Green, 1 = Red, 2 = Orange, 3 = Amber, 4 = Yellow, 5 = Lime Green, 6 = Spring Green, 7 = Cyan, 8 = Sky Blue, 9 = Blue, 10 = Violet, 11 = Magenta, 12 = Rose, 13 = White, 14 = Custom1, 15 = Custom2 | 0 |  |  |  | Color 1 | The main color of the Animation, Custom Colors are defined in Parameter data
11 | 53 | 3-bit UInteger | 0 = High, 1 = Medium, 2 = Low, 3 = Off, 4 = Custom | 0 |  |  |  | Color 1 Intensity | The Intensity of Color 1, Custom Intensity defined in Parameter Data
12 | 56 | 5-bit UInteger | 0 = Green, 1 = Red, 2 = Orange, 3 = Amber, 4 = Yellow, 5 = Lime Green, 6 = Spring Green, 7 = Cyan, 8 = Sky Blue, 9 = Blue, 10 = Violet, 11 = Magenta, 12 = Rose, 13 = White, 14 = Custom1, 15 = Custom2 | 0 |  |  |  | Color 2 | The secondary color of the Animation, Custom Colors are defined in Parameter data
13 | 61 | 3-bit UInteger | 0 = High, 1 = Medium, 2 = Low, 3 = Off, 4 = Custom | 0 |  |  |  | Color 2 Intensity | The Intensity of Color 2, Custom Intensity defined in Parameter Data

Octet 0

bit offset | 63 | 62 | 61 | 60 | 59 | 58 | 57 | 56
subindex | 13 | 12
element bit | 2 | 1 | 0 | 4 | 3 | 2 | 1 | 0

Octet 1

bit offset | 55 | 54 | 53 | 52 | 51 | 50 | 49 | 48
subindex | 11 | 10
element bit | 2 | 1 | 0 | 4 | 3 | 2 | 1 | 0

Octet 2

bit offset | 47 | 46 | 45 | 44 | 43 | 42 | 41 | 40
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 9
element bit |  |  |  |  |  | 2 | 1 | 0

Octet 3

bit offset | 39 | 38 | 37 | 36 | 35 | 34 | 33 | 32
subindex | 8
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 4

bit offset | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
subindex | 7
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 5

bit offset | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
subindex | 7
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 6

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | 6 | 5 | 4
element bit |  |  |  |  | 1 | 0 | 1 | 0

Octet 7

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | 3 | 2 | 1
element bit | 2 | 1 | 0 |  | 3 | 2 | 1 | 0

## Variable "Custom Color 1" index=88 id=V_CustomColor1Configuration

description: Custom Color 1
data type: 24-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0..255 | 255 |  |  |  | Red | Red value for custom color
2 | 8 | 8-bit UInteger | 0..255 | 255 |  |  |  | Green | Green value for custom color
3 | 16 | 8-bit UInteger | 0..255 | 255 |  |  |  | Blue | Blue value for custom color

octet | 0 | 1 | 2 |
bit offset | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 2 | 1 |
element bit | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Custom Color 2" index=89 id=V_CustomColor2Configuration

description: Custom Color 2
data type: 24-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0..255 | 255 |  |  |  | Red | Red value for custom color
2 | 8 | 8-bit UInteger | 0..255 | 255 |  |  |  | Green | Green value for custom color
3 | 16 | 8-bit UInteger | 0..255 | 255 |  |  |  | Blue | Blue value for custom color

octet | 0 | 1 | 2 |
bit offset | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 2 | 1 |
element bit | 7 - 0 | 7 - 0 | 7 - 0 |

[Top]

## ErrorTypes

Code | Additional code | Name | Description
--- | --- | --- | ---
128 (0x80) | 0 (0x00) | Device application error - no details | Service has been refused by the device application and no detailed information of the incident is available
128 (0x80) | 17 (0x11) | Index not available | Access occurs to a not existing index
128 (0x80) | 18 (0x12) | Subindex not available | Access occurs to a not existing subindex
128 (0x80) | 32 (0x20) | Service temporarily not available | Parameter is not accessible due to the current state of the device application
128 (0x80) | 35 (0x23) | Access denied | Write access on a read-only parameter
128 (0x80) | 48 (0x30) | Parameter value out of range | Written parameter value is outside its permitted value range
128 (0x80) | 49 (0x31) | Parameter value above limit | Written parameter value is above its specified value range
128 (0x80) | 51 (0x33) | Parameter length overrun | Written parameter length is above its predefined length
128 (0x80) | 52 (0x34) | Parameter length underrun | Written parameter length is below its predefined length
128 (0x80) | 53 (0x35) | Function not available | Written command is not supported by the device application
128 (0x80) | 54 (0x36) | Function temporarily unavailable | Written command is not available due to the current state of the device application
128 (0x80) | 65 (0x41) | Inconsistent parameter set | Parameter inconsistencies were found at the end of block parameter transfer, device plausibility check failed

[Top]

## Events

Code | Type | Name | Description
--- | --- | --- | ---
0 (0x0000) | Notification | No malfunction |
20480 (0x5000) | Error | Device hardware fault | Device Exchange

[Top]

## Observer Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_SerialNumber
V_HardwareRevision
V_FirmwareRevision
V_ApplicationSpecificTag

Parameter Menu
Executable Commands
V_SystemCommand, Button:=130 Description=Factory Reset
Device Access Locks
V_DeviceAccessLocks.Parameter (write) Access Lock
V_DeviceAccessLocks.Data Storage Lock
Operation Mode
V_OperationMode
State 1 Parameters
V_StateParameters1.Animation Type, Dec
V_StateParameters1.Animation Direction, Dec
V_StateParameters1.Animation Pattern, Dec
V_StateParameters1.Animation Speed, Dec
V_StateParameters1.Vibration Feedback, Dec
V_StateParameters1.Off Delay Type, Dec
V_StateParameters1.Off Delay (ms) ms, Dec
V_StateParameters1.Static Sequence Value (0-255), Dec
V_StateParameters1.Sequence Start Location, Dec
V_StateParameters1.Color 1, Dec
V_StateParameters1.Color 1 Intensity, Dec
V_StateParameters1.Color 2, Dec
V_StateParameters1.Color 2 Intensity, Dec
State 2 Parameters
V_StateParameters2.Animation Type, Dec
V_StateParameters2.Animation Direction, Dec
V_StateParameters2.Animation Pattern, Dec
V_StateParameters2.Animation Speed, Dec
V_StateParameters2.Vibration Feedback, Dec
V_StateParameters2.Off Delay Type, Dec
V_StateParameters2.Off Delay (ms) ms, Dec
V_StateParameters2.Static Sequence Value (0-255), Dec
V_StateParameters2.Sequence Start Location, Dec
V_StateParameters2.Color 1, Dec
V_StateParameters2.Color 1 Intensity, Dec
V_StateParameters2.Color 2, Dec
V_StateParameters2.Color 2 Intensity, Dec
State 3 Parameters
V_StateParameters3.Animation Type, Dec
V_StateParameters3.Animation Direction, Dec
V_StateParameters3.Animation Pattern, Dec
V_StateParameters3.Animation Speed, Dec
V_StateParameters3.Vibration Feedback, Dec
V_StateParameters3.Off Delay Type, Dec
V_StateParameters3.Off Delay (ms) ms, Dec
V_StateParameters3.Static Sequence Value (0-255), Dec
V_StateParameters3.Sequence Start Location, Dec
V_StateParameters3.Color 1, Dec
V_StateParameters3.Color 1 Intensity, Dec
V_StateParameters3.Color 2, Dec
V_StateParameters3.Color 2 Intensity, Dec
State 4 Parameters
V_StateParameters4.Animation Type, Dec
V_StateParameters4.Animation Direction, Dec
V_StateParameters4.Animation Pattern, Dec
V_StateParameters4.Animation Speed, Dec
V_StateParameters4.Vibration Feedback, Dec
V_StateParameters4.Off Delay Type, Dec
V_StateParameters4.Off Delay (ms) ms, Dec
V_StateParameters4.Static Sequence Value (0-255), Dec
V_StateParameters4.Sequence Start Location, Dec
V_StateParameters4.Color 1, Dec
V_StateParameters4.Color 1 Intensity, Dec
V_StateParameters4.Color 2, Dec
V_StateParameters4.Color 2 Intensity, Dec
Touch Settings
V_InputSettings.Touch Sensitivity, Dec
V_InputSettings.Function, Dec
V_InputSettings.Mute Enable, Dec
V_InputSettings.On Delay (ms) ms, Dec
Output Settings
V_OutputSettings.Output State, Dec
V_OutputSettings.Off Delay Type, Dec
V_OutputSettings.Off Delay (ms) ms, Dec
Custom Animation Settings
V_CustomAnimationSettings.Custom Intensity (0 - 100%) %, Dec
V_CustomAnimationSettings.Custom Flash Rate (0.5 - 25.5 Hz) * 0.1 Hz, Dec
V_CustomAnimationSettings.Restrict To Gamut, Dec
Custom Color 1 Configuration
V_CustomColor1Configuration.Red, Dec
V_CustomColor1Configuration.Green, Dec
V_CustomColor1Configuration.Blue, Dec
Custom Color 2 Configuration
V_CustomColor2Configuration.Red, Dec
V_CustomColor2Configuration.Green, Dec
V_CustomColor2Configuration.Blue, Dec

## Maintenance Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_SerialNumber
V_HardwareRevision
V_FirmwareRevision
V_ApplicationSpecificTag

Parameter Menu
Executable Commands
V_SystemCommand, Button:=130 Description=Factory Reset
Device Access Locks
V_DeviceAccessLocks.Parameter (write) Access Lock
V_DeviceAccessLocks.Data Storage Lock
Operation Mode
V_OperationMode
State 1 Parameters
V_StateParameters1.Animation Type, Dec
V_StateParameters1.Animation Direction, Dec
V_StateParameters1.Animation Pattern, Dec
V_StateParameters1.Animation Speed, Dec
V_StateParameters1.Vibration Feedback, Dec
V_StateParameters1.Off Delay Type, Dec
V_StateParameters1.Off Delay (ms) ms, Dec
V_StateParameters1.Static Sequence Value (0-255), Dec
V_StateParameters1.Sequence Start Location, Dec
V_StateParameters1.Color 1, Dec
V_StateParameters1.Color 1 Intensity, Dec
V_StateParameters1.Color 2, Dec
V_StateParameters1.Color 2 Intensity, Dec
State 2 Parameters
V_StateParameters2.Animation Type, Dec
V_StateParameters2.Animation Direction, Dec
V_StateParameters2.Animation Pattern, Dec
V_StateParameters2.Animation Speed, Dec
V_StateParameters2.Vibration Feedback, Dec
V_StateParameters2.Off Delay Type, Dec
V_StateParameters2.Off Delay (ms) ms, Dec
V_StateParameters2.Static Sequence Value (0-255), Dec
V_StateParameters2.Sequence Start Location, Dec
V_StateParameters2.Color 1, Dec
V_StateParameters2.Color 1 Intensity, Dec
V_StateParameters2.Color 2, Dec
V_StateParameters2.Color 2 Intensity, Dec
State 3 Parameters
V_StateParameters3.Animation Type, Dec
V_StateParameters3.Animation Direction, Dec
V_StateParameters3.Animation Pattern, Dec
V_StateParameters3.Animation Speed, Dec
V_StateParameters3.Vibration Feedback, Dec
V_StateParameters3.Off Delay Type, Dec
V_StateParameters3.Off Delay (ms) ms, Dec
V_StateParameters3.Static Sequence Value (0-255), Dec
V_StateParameters3.Sequence Start Location, Dec
V_StateParameters3.Color 1, Dec
V_StateParameters3.Color 1 Intensity, Dec
V_StateParameters3.Color 2, Dec
V_StateParameters3.Color 2 Intensity, Dec
State 4 Parameters
V_StateParameters4.Animation Type, Dec
V_StateParameters4.Animation Direction, Dec
V_StateParameters4.Animation Pattern, Dec
V_StateParameters4.Animation Speed, Dec
V_StateParameters4.Vibration Feedback, Dec
V_StateParameters4.Off Delay Type, Dec
V_StateParameters4.Off Delay (ms) ms, Dec
V_StateParameters4.Static Sequence Value (0-255), Dec
V_StateParameters4.Sequence Start Location, Dec
V_StateParameters4.Color 1, Dec
V_StateParameters4.Color 1 Intensity, Dec
V_StateParameters4.Color 2, Dec
V_StateParameters4.Color 2 Intensity, Dec
Touch Settings
V_InputSettings.Touch Sensitivity, Dec
V_InputSettings.Function, Dec
V_InputSettings.Mute Enable, Dec
V_InputSettings.On Delay (ms) ms, Dec
Output Settings
V_OutputSettings.Output State, Dec
V_OutputSettings.Off Delay Type, Dec
V_OutputSettings.Off Delay (ms) ms, Dec
Custom Animation Settings
V_CustomAnimationSettings.Custom Intensity (0 - 100%) %, Dec
V_CustomAnimationSettings.Custom Flash Rate (0.5 - 25.5 Hz) * 0.1 Hz, Dec
V_CustomAnimationSettings.Restrict To Gamut, Dec
Custom Color 1 Configuration
V_CustomColor1Configuration.Red, Dec
V_CustomColor1Configuration.Green, Dec
V_CustomColor1Configuration.Blue, Dec
Custom Color 2 Configuration
V_CustomColor2Configuration.Red, Dec
V_CustomColor2Configuration.Green, Dec
V_CustomColor2Configuration.Blue, Dec

## Specialist Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_SerialNumber
V_HardwareRevision
V_FirmwareRevision
V_ApplicationSpecificTag

Parameter Menu
Executable Commands
V_SystemCommand, Button:=130 Description=Factory Reset
Device Access Locks
V_DeviceAccessLocks.Parameter (write) Access Lock
V_DeviceAccessLocks.Data Storage Lock
Operation Mode
V_OperationMode
State 1 Parameters
V_StateParameters1.Animation Type, Dec
V_StateParameters1.Animation Direction, Dec
V_StateParameters1.Animation Pattern, Dec
V_StateParameters1.Animation Speed, Dec
V_StateParameters1.Vibration Feedback, Dec
V_StateParameters1.Off Delay Type, Dec
V_StateParameters1.Off Delay (ms) ms, Dec
V_StateParameters1.Static Sequence Value (0-255), Dec
V_StateParameters1.Sequence Start Location, Dec
V_StateParameters1.Color 1, Dec
V_StateParameters1.Color 1 Intensity, Dec
V_StateParameters1.Color 2, Dec
V_StateParameters1.Color 2 Intensity, Dec
State 2 Parameters
V_StateParameters2.Animation Type, Dec
V_StateParameters2.Animation Direction, Dec
V_StateParameters2.Animation Pattern, Dec
V_StateParameters2.Animation Speed, Dec
V_StateParameters2.Vibration Feedback, Dec
V_StateParameters2.Off Delay Type, Dec
V_StateParameters2.Off Delay (ms) ms, Dec
V_StateParameters2.Static Sequence Value (0-255), Dec
V_StateParameters2.Sequence Start Location, Dec
V_StateParameters2.Color 1, Dec
V_StateParameters2.Color 1 Intensity, Dec
V_StateParameters2.Color 2, Dec
V_StateParameters2.Color 2 Intensity, Dec
State 3 Parameters
V_StateParameters3.Animation Type, Dec
V_StateParameters3.Animation Direction, Dec
V_StateParameters3.Animation Pattern, Dec
V_StateParameters3.Animation Speed, Dec
V_StateParameters3.Vibration Feedback, Dec
V_StateParameters3.Off Delay Type, Dec
V_StateParameters3.Off Delay (ms) ms, Dec
V_StateParameters3.Static Sequence Value (0-255), Dec
V_StateParameters3.Sequence Start Location, Dec
V_StateParameters3.Color 1, Dec
V_StateParameters3.Color 1 Intensity, Dec
V_StateParameters3.Color 2, Dec
V_StateParameters3.Color 2 Intensity, Dec
State 4 Parameters
V_StateParameters4.Animation Type, Dec
V_StateParameters4.Animation Direction, Dec
V_StateParameters4.Animation Pattern, Dec
V_StateParameters4.Animation Speed, Dec
V_StateParameters4.Vibration Feedback, Dec
V_StateParameters4.Off Delay Type, Dec
V_StateParameters4.Off Delay (ms) ms, Dec
V_StateParameters4.Static Sequence Value (0-255), Dec
V_StateParameters4.Sequence Start Location, Dec
V_StateParameters4.Color 1, Dec
V_StateParameters4.Color 1 Intensity, Dec
V_StateParameters4.Color 2, Dec
V_StateParameters4.Color 2 Intensity, Dec
Touch Settings
V_InputSettings.Touch Sensitivity, Dec
V_InputSettings.Function, Dec
V_InputSettings.Mute Enable, Dec
V_InputSettings.On Delay (ms) ms, Dec
Output Settings
V_OutputSettings.Output State, Dec
V_OutputSettings.Off Delay Type, Dec
V_OutputSettings.Off Delay (ms) ms, Dec
Custom Animation Settings
V_CustomAnimationSettings.Custom Intensity (0 - 100%) %, Dec
V_CustomAnimationSettings.Custom Flash Rate (0.5 - 25.5 Hz) * 0.1 Hz, Dec
V_CustomAnimationSettings.Restrict To Gamut, Dec
Custom Color 1 Configuration
V_CustomColor1Configuration.Red, Dec
V_CustomColor1Configuration.Green, Dec
V_CustomColor1Configuration.Blue, Dec
Custom Color 2 Configuration
V_CustomColor2Configuration.Red, Dec
V_CustomColor2Configuration.Green, Dec
V_CustomColor2Configuration.Blue, Dec

Note: This page shows the content of an IODD file transformed into HTML format. In the case of disparity between this and the XML view, the content of the XML file takes precedence.
Created by IODD Viewer V1.1.